COST EXTENDED HATA MODEL TAB HELP

Enter base station antenna height, mobile station antenna
height, TX/RX distance, frequency, and area type, then
click Calculate.

Valid Input:
  Frequency: 1500 MHz to 2000 MHz
  Base Station Height: 30 m to 200 m (98.43 ft to 656.17 ft)
  Mobile Station Height: 1 m to 10 m (3.28 ft to 32.81 ft)
  Distance: 1 km to 10 km (0.62 mi to 6.21 mi)
  Area Type: Suburban or Metropolitan

Features:
  - Forward and reverse calculation modes
  - Apply and Graph buttons

The COST 231 Extended Hata model extends the original
Hata model to the PCS frequency range (1500-2000 MHz).
It is recommended for urban and suburban propagation
studies in the 1.5 to 2 GHz band.
