HATA MODEL (OPEN) TAB HELP

Same input parameters as the Hata Urban model.

Valid Input:
  Frequency: 150 MHz to 1500 MHz
  Base Station Height: 30 m to 200 m (98.43 ft to 656.17 ft)
  Mobile Station Height: 1 m to 10 m (3.28 ft to 32.81 ft)
  Distance: 1 km to 100 km (0.62 mi to 62.14 mi)

The Hata Open model is designed for wide-open areas
completely outside the city, such as farmland or open
plains. It uses the Hata Urban output as a base and
applies an open-area correction factor.
