WEISSBERGER'S MODEL TAB HELP

Enter the depth of foliage obstruction, TX/RX distance,
and transmission frequency, then click Calculate.

Valid Input:
  Foliage Depth: 0 m to 400 m (0 ft to 1312.34 ft)
  TX/RX Distance: 0.001 km to 500 km (0.0007 mi to 310.69 mi)
  Frequency: 230 MHz to 95 GHz

Features:
  - Forward and reverse calculation modes
  - Apply and Graph buttons

Weissberger's model calculates path loss for line-of-sight
links that are obstructed by foliage (trees, dense vegetation).
It is most accurate for frequencies between 230 MHz and 95 GHz.
