COST-W-I MODEL (NLoS) TAB HELP

Enter transmitter height, receiver height, TX/RX distance,
frequency, mean building height, mean street width, mean
building separation, and road orientation angle.

Valid Input:
  Transmitter Height: 4 m to 50 m (13.12 ft to 164.04 ft)
  Receiver Height: 1 m to 3 m (3.28 ft to 9.84 ft)
  TX/RX Distance: 0.02 km to 5 km (0.0125 mi to 3.11 mi)
  Frequency: 800 MHz to 2000 MHz
  Building Height: Positive numeric value
  Street Width: Positive numeric value
  Building Separation: Positive numeric value
  Road Orientation: 0 to 90 degrees

The COST-Walfisch-Ikegami (Non-Line-of-Sight) model is an
empirical model designed for cellular and PCS propagation
prediction in urban microcell environments where there is
no direct line of sight between transmitter and receiver.
