HATA MODEL (SUBURBAN) TAB HELP

Same input parameters as the Hata Urban model.

Valid Input:
  Frequency: 150 MHz to 1500 MHz
  Base Station Height: 30 m to 200 m (98.43 ft to 656.17 ft)
  Mobile Station Height: 1 m to 10 m (3.28 ft to 32.81 ft)
  Distance: 1 km to 100 km (0.62 mi to 62.14 mi)

The Hata Suburban model is designed for areas just outside
cities and rural areas with man-made structures that are
less dense than urban environments. It uses the Hata Urban
output as a base and applies a suburban correction factor.
