COST-W-I MODEL (LoS) TAB HELP

Enter TX/RX distance and frequency, then click Calculate.

Valid Input:
  TX/RX Distance: 0.02 km to 5 km (0.0125 mi to 3.11 mi)
  Frequency: 800 MHz to 2000 MHz

Features:
  - Forward and reverse calculation modes
  - Apply and Graph buttons

The COST-Walfisch-Ikegami (Line-of-Sight) model is the
line-of-sight version of the COST-W-I model, used for
cellular and PCS propagation prediction when a clear
line of sight exists between transmitter and receiver.
