HATA MODEL (URBAN) TAB HELP

Enter the base station antenna height, mobile station antenna
height, TX/RX distance, frequency, and city type, then click
Calculate.

Valid Input:
  Frequency: 150 MHz to 1500 MHz
  Base Station Height: 30 m to 200 m (98.43 ft to 656.17 ft)
  Mobile Station Height: 1 m to 10 m (3.28 ft to 32.81 ft)
  Distance: 1 km to 100 km (0.62 mi to 62.14 mi)
  City Type: Large or Small/Medium

Features:
  - Forward and reverse calculation modes
  - Apply and Graph buttons

The Hata Urban model (Okumura-Hata) is one of the most widely
used empirical propagation models for cellular communication.
It applies to urban macrocell environments. The extended range
uses ITU-R P.529-3 to allow distances beyond the original 20 km.
